# GGSN APN Generic

The GGSN APN Generic category of the Chassis Configuration dialog box lists the access point system information.

Note This dialog can be viewed if cGtpGSNService is set to 'ggsn'.

## Procedure

1. Right-click the device and then select Configure, or double-click the device.

2. Select GGSN APN Generic from the Category list.

The following information appears:

Notification Controller (cgprsAccPtCfgNotifEnable)

Max History Table Size (cgprsAccPtCfgNotifHistMax)

Latest Entries Index (cgprsAccPtCfgNotifLatestIndex)

### Notification Controller (cgprsAccPtCfgNotifEnable)

Controls the generation of cgprsAccPtCfgNotif notifications. However, entries in the cgprsAccPtCfgNotifHistTable are generated irrespective of the value of this object.

### Max History Table Size (cgprsAccPtCfgNotifHistMax)

Maximum number of entries in the event history table cgprsAccPtCfgNotifHistTable.

When the table is full, the oldest entries are removed to make space for new entries.

### Latest Entries Index (cgprsAccPtCfgNotifLatestIndex)

Value of cgprsAccPtCfgNotifIndex for the most recently created entry in cgprsAccPtCfgNotifHistTable.

###