# Monitor MAC Layer Traffic

Use this option to monitor packet count for a source and destination address or monitor packet count for a souce or destination address on a particular SRP interface.

## Procedure

To access monitor MAC layer traffic information:

1. Right-click the port and select SRP Interface Statistics from the pop-up menu.

MAC Layer Traffic dialog box appears.

2. Select Monitor MAC Layer Traffic from the Category menu to display monitor MAC layer traffic information.

Monitor MAC Layer Traffic dialog box displays:

Packets Received (srpMACCountPktsBySource)

Packets Sent (srpMACCountPktsByDest)

### Packets Received (srpMACCountPktsBySource)

Number of packets received from a source node MAC address.

Discontinuities in value can occur at management system reinitialization depending on the srpMACSourceDiscontTimeStamp.

### Packets Sent (srpMACCountPktsByDest)

Number of packets sent to a node MAC address.

Discontinuities in value can occur at management system reinitialization depending on the srpMACSourceDiscontTimeStamp.

## Related Topics

Using CiscoView Interface

Using the Main Menu

Selecting Components

Configuring Devices and Components

Monitoring Devices and Components