# IP Port Address Table

To access the dialog box:

> 1. Right-click the device, and select Configure from the popup menu. Device configuration information appears.

> 2. Select IP Table from the Category drop-down list box.

The following information appears:

> Port (ipAdEntIfIndex)

> Description (ifDescr)

> IP Address(ipAdEntAddr)

> Subnet Mask(ipAdEntNetMask)

> Broadcast Format (ipAdEntBcastAddr)

Port (ipAdEntIfIndex)

Specifies the interface number.

Description (ifDescr)

A textual string containing information about the interface. This string should include the name of the manufacturer, the product name, and the version of the interface hardware/software.

IP Address (ipAdEntAddr)

Specifies the 32-bit IP address for this entry.

Subnet Mask (ipAdEntNetMask)

Specifies the subnet mask for the IP address.

Broadcast Format (ipAdEntBcastAddr)

Specifies the broadcast format for the interface. Possible values are 1 for the all-1s format or 0 for the all-0s format.