# CDMA PDSN IP Flows Table

The table displays following information:

IpAddress (cCdmaSessionUserFlowIpAddress)

N/W Access ID (cCdmaSessionNai)

Addressing Scheme (cCdmaSessionAddressingScheme)

Flow Technology (cCdmaSessionFlowTechnology)

HA IpAddress (cCdmaSessionHaIpAddress)

Tunneling Protocol (cCdmaSessionTunnelProt)

### IpAddress(cCdmaSessionUserFlowIpAddress)

User flow IP address.

### N/W Access ID(cCdmaSessionNai)

User's network access identifier. User@domain construct, which identifies home network of mobile user.

### Addressing Scheme(cCdmaSessionAddressingScheme)

Mobile station IP address type.

Values are:

other (1) |
static (2) | Mobile station has a static IP address configured.
dynamic (3) | Mobile station is dynamically assigned an IP address.

### Flow Technology(cCdmaSessionFlowTechnology)

Routing technology used by a flow.

Values are:

other (1) |
simpleIP (2) | IP routing.
mobileIP (3) | Mobile IP routing.
proxymobileIP (4) | MoIP routing with PDSN acting as a proxy MC.

### HA IpAddress(cCdmaSessionHaIpAddress)

Mobile IP home agent address.

Note: Relevant only if MoIP or Proxy MoIP is used.

### Tunneling Protocol(cCdmaSessionTunnelProt)

Tunneling protocol used between mobile station and packet data serving node.

Values are:

other (1) | other protocol.
notunnel (2) | no tunnel encapsulation.
12tp (3) | tunnel encapsulation using 12tp protocol.
12f (4) | tunnel encapsulation using 12f protocol.
mobileip (5) | tunnel encapsulation using GRE protocol.