# CDMA PDSN Cluster Member Table

The PDSN Cluster Member Table category of the Device Configuration dialog box allows you to view the packet data servicing node (PDSN) cluster member details.

## Procedure

1. Right-click the device, then select Configure or double-click the device. The Device Configuration dialog box appears.

2. Select PDSN Cluster Member Table from the Category list.

The following information appears:

Cluster Member Address Type (cCdmaClusterMemberAddressType)

Cluster Member Address (cCdmaClusterMemberAddress)

Cluster Member Status (cCdmaClusterMemberStatus)

Cluster Member Load (cCdmaClusterMemberLoad)

### Cluster Member Address Type (cCdmaClusterMemberAddressType)

IP address type of the the packet data servicing node (PDSN) cluster member. The address type is combined with the cluster member address and used as an index to identify a unique cluster member entry.

### Cluster Member Address (cCdmaClusterMemberAddress)

IP address of the the packet data servicing node (PDSN) cluster member. The address is combined with the cluster member address type and used as an index to identify a unique cluster member entry.

### Cluster Member Status (cCdmaClusterMemberStatus)

Operational status of the packet data servicing node (PDSN). Status can be:

Value | Description
1 | unknown - Cluster controller does not know the member status.
2 | ready - Member is ready to serve call setup request.
3 | adminProhibit - Member does not request for new call setup, but maintains existing calls.

### Cluster Member Load (cCdmaClusterMemberLoad)

Packet data servicing node (PDSN) cluster member load as an aggregate percentage of the maximum load that can be serviced.