# CDMA PDSN PPP Setup Failures

From this dialog box, you can view the PPP requests that have been rejected.

## Navigation

1. Right-click the Mobile Wireless Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN PPP Setup Failures.

The following information is displayed:

> PPP Connection Setup Reqs Failed (cCdmaPppConnectionFailures)

> PPP Connections Failed at LCP stage (cCdmaPppLcpFailures)

> PPP Connections Failed at AUTH stage (cCdmaPppAuthFailures)

> PPP Connections Failed at IPCP stage (cCdmaPppIpcpFailures)

> The following objects are available only in PDSN 2.0:

> LCP Stage Failures after Maximum Retransmissions (cCdmaPppLcpFailuresMaxRetrans)

> LCP Stage Failures Due to Unknown Reason (cCdmaPppLcpFailuresUnknown)

> IPCP Stage Failures after Maximum Retransmissions (cCdmaPppIpcpFailuresMaxRetrans)

> IPCP Stage Failures Due to Unknown Reason (cCdmaPppIpcpFailuresUnknown)

> PPP Negotiations Aborted Prematurely (cCdmaPppConnectionsAborted)

### PPP Connection Setup Reqs Failed (cCdmaPppConnectionFailures)

Number of times PPP connection setup requests failed since system startup.

### PPP Connections Failed at LCP stage (cCdmaPppLcpFailures)

Number of times PPP connection requests failed at the LCP stage since system startup.

### PPP Connections Failed at AUTH stage (cCdmaPppAuthFailures)

Number of times PPP setup connections failed at the authentication stage since system startup.

### PPP Connections Failed at IPCP stage (cCdmaPppIpcpFailures)

Number of times PPP setup connections failed at the IPCP stage since system startup.

### LCP Stage Failures after Maximum Retransmissions (cCdmaPppLcpFailuresMaxRetrans)

Number of PPP connection requests that failed at the LCP stage after the maximum number of retransmissions was reached since system startup.

### LCP Stage Failures Due to Unknown Reason (cCdmaPppLcpFailuresUnknown)

Number of PPP connection requests that failed at the LCP stage because of an unknown reason since system startup.

### IPCP Stage Failures after Maximum Retransmissions (cCdmaPppIpcpFailuresMaxRetrans)

Number of PPP connection requests that failed at the IPCP stage after the maximum number of retransmissions was reached since system startup.

### IPCP Stage Failures Due to Unknown Reason (cCdmaPppIpcpFailuresUnknown)

Number of PPP connection requests that failed at the IPCP stage because of an unknown reason since system startup.

### PPP Negotiations Aborted Prematurely (cCdmaPppConnectionsAborted)

Number of PPP negotiations that terminated prematurely due to a module node (MN) power-off since system startup.