# Foreign Agent Visitors List

## Navigation

1. Right-click the device, and select Configure. The Device Configuration dialog box appears.
2. Select Foreign Agent Visitors List from the Category list.

The following information appears:

> Visitor Identifier Type (cmiFaRegVisitorIdentifierType)

> Visitor Identifier Associated (cmiFaRegVisitorIdentifier)

> Home IP Address (cmiFaRegVisitorHomeAddress)

> Home Agent IP Address (cmiFaRegVisitorHomeAgentAddress)

> Lifetime (cmiFaRegVisitorTimeGranted)

> Time to Expire (cmiFaRegVisitorTimeRemaining)

> ID Low Bits (cmiFaRegVisitorRegIDLow)

> ID High Bits (cmiFaRegVisitorRegIDHigh)

> Registration Acceptance (cmiFaRegVisitorRegIsAccepted)

> Challenge Value (cmiFaRegVisitorChallengeValue)

> Visitor Registration Flags (CmiFaRegVisitorRegFlagsRev1)

### Visitor Identifier Type (cmiFaRegVisitorIdentifierType)

The type of the visitor's identifier.

### Visitor Identifier Associated (cmiFaRegVisitorIdentifier)

The identifier associated with the visitor.

### Home IP Address (cmiFaRegVisitorHomeAddress)

The home (IP) address of the visiting mobile node.

### Home Agent IP Address (cmiFaRegVisitorHomeAgentAddress)

The home agent IP address for that visiting mobile node.

### Lifetime (cmiFaRegVisitorTimeGranted)

The lifetime granted to the mobile node for this registration. Only valid if faVisitorRegIsAccepted is true (1).

### Time to Expire (cmiFaRegVisitorTimeRemaining)

The time remaining until the registration expires. It has the same initial value as cmiFaRegVisitorTimeGranted and is counted down by the foreign agent.

### ID Low Bits (cmiFaRegVisitorRegIDLow)

Low 32 bits of identification used in that registration by the mobile node.

### ID High Bits (cmiFaRegVisitorRegIDHigh)

High 32 bits of identification used in that registration by the mobile node.

### Registration Acceptance (cmiFaRegVisitorRegIsAccepted)

Indicates whether the registration has been accepted or not. If it is false (2), this registration is still pending for reply.

### Challenge Value (cmiFaRegVisitorChallengeValue)

The challenge value forwarded to the mobile node in the previous registration reply, which can be used by the mobile node in the next registration request.

### Visitor Registration Flags (CmiFaRegVisitorRegFlagsRev1)

Registration flags sent by the mobile node.