# Monitoring the Device Environment

The CiscoView Monitor Device window displays the following environment information.

Use this option to view status information for GGSN.

## Procedure

1. Right-click the device, and select Monitor.

2. Select Environment from the Category list.

The following information appears for the device you are managing:

Airflow Temp In

Airflow Temp Out

+3.45 Volt

+5.15 Volt

+12.15 Volt

-11.95 Volt

Airflow Temp In

Displays the current temperature of air entering the router (Cisco 7000).

Airflow Temp Out

Displays the temperature of the exhaust airflow of the router (Cisco 7000).

+3.45 Volt

Displays the current value (in millivolts) for the +3.45V line from the power supply on the router (Cisco 7000).

+5.15 Volt (envTestPt3Measure)

Displays the current value (in millivolts) for the +5.15V line from the power supply on the router (Cisco 7000).

+12.15 Volt (envTestPt4Measure)

Displays the current value (in millivolts) of the +12.15V line from the power supply of the router.

-11.95 Volt

Displays the current value (in millivolts) of the -11.95 line from the power supply of the router.