# Mobile IP Security Violation Configs

## Navigation

1. Right-click the device, and select Configure. The Device Configuration dialog box appears.

2. Select Mobile IP Security Violation Configs from the Category list.

The following information appears:

> Security Violator's Identifier Type (cmiSecViolatorIdentifierType)

> Security Violator's Identifier (cmiSecViolatorIdentifier)

> Recent Security Violation SPI (cmiSecRecentViolationSPI)

> Recent Security Violation Time (cmiSecRecentViolationTime)

> Lower Order Identification Bits (cmiSecRecentViolationIDLow)

> Higher Order Identification Bits (cmiSecRecentViolationIDHigh)

> Recent Security Violation Reason (cmiSecRecentViolationReason)

### Security Violator's Identifier Type (cmiSecViolatorIdentifierType)

The type of violator's identifier.

### Security Violator's Identifier (cmiSecViolatorIdentifier)

The violator's identifier. The violator is not necessary in the cmiSecAssocTable.

### Recent Security Violation SPI (cmiSecRecentViolationSPI)

The SPI of the most recent security violation for this peer. If the security violation is due to:

- An identification mismatch, then this is the SPI from the Mobile-Home Authentication Extension.
- An invalid authenticator, then this is the SPI from the offending authentication extension.

In all other cases, it should be set to zero.

### Recent Security Violation Time (cmiSecRecentViolationTime)

The time of the most recent security violation for this peer.

### Lower Order Identification Bits (cmiSecRecentViolationIDLow)

Low-order 32 bits of identification used in request or reply of the most recent security violation for this peer.

### Higher Order Identification Bits (cmiSecRecentViolationIDHigh)

High-order 32 bits of identification used in request or reply of the most recent security violation for this peer.

### Recent Security Violation Reason (cmiSecRecentViolationReason)

The reason for the most recent security violation for this peer.