# Charging Gateway Table for GGSN

The table displays the following information:

IP Address (cgprsGtpChargingGWid)

Name (cgprsGtpChargingGWName)

Type (cgprsGtpChargingGWType)

Operation State (cgprsGtpChargingGWOperState)

Charging Gateway Up-Down Trap Enable (cgprsGtpChargingGWNotifEnable)

Row Status (cgprsGtpChargingGWRowStatus)

### IP Address (cgprsGtpChargingGWid)

Specifies the IP address being used by the unique charging gateway.

### Name (cgprsGtpChargingGWName)

Indicates the name of the charging gateway.

### Type (cgprsGtpChargingGWType)

Indicates the type of charging gateway being used. The value can be set to 'primary' if the gateway is a primary charging gateway. A primary charging gateway and one backup charging gateway are used.

The default is 'primary'.

### Operation State (cgprsGtpChargingGWOperState)

Indicates the operating state of the charging gateway

Value | Description
Up | Charging gateway is up.
Down | Charging gateway is down.
Unknown | Charging gateway state can not be determined, for example, from the time the gateway and actual state is detected as functional.

### Charging Gateway Up-Down Trap Enable (cgprsGtpChargingGWNotifEnable)

Indicates whether the system produces the cgprsGtpCharginGWNotif.

### Row Status (cgprsGtpChargingGWRowStatus)

Indicates the status of the row. The value is considered to create and delete a row in the table.