# Active Call Monitor

The Active Call Monitor dialog box provides you the details of an active call.

## Procedure

1. In the rear view, right-click the LEDs of FXS ports available in the CMM submodule.

2. Select Active Call Status from the popup menu. The Active Call Status dialog box appears.

3. Click Monitor.

The following information appears:

> Transmit Packets (callActiveTransmitPackets)

> Transmit Bytes (callActiveTransmitBytes)

> Receive Packets (callActiveReceivePackets)

> Receive Bytes (callActiveReceiveBytes)

### Transmit Packets (callActiveTransmitPackets)

The number of packets that are transmitted for this call.

### Transmit Bytes (callActiveTransmitBytes)

The number of bytes that are transmitted for this call.

### Receive Packets (callActiveReceivePackets)

The number of packets that are received for this call.

### Receive Bytes (callActiveReceiveBytes)

The number of bytes that are received for this call.