# GGSN CAC Virtual BW Pool

## Procedure

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select GGSN CAC Virtual BW Pool from the Category drop-down box.

The following information appears:

> Virtual BW Pool Name (cggsnUmtsQosCacBWPoolName)

> Total Bandwidth (cggsnUmtsQosCacBWPoolBWVal)

### Virtual BW Pool Name (cggsnUmtsQosCacBWPoolName)

Name of the virtual bandwidth pool which will be attached to the Access Point Name (APN).

### Total Bandwidth (cggsnUmtsQosCacBWPoolBWVal)

Indicates the total bandwidth for this pool.

Note: A value for this object must be set for each table entry.