# GGSN Access Point CAC Configuration

## Procedure

1. Right-click the device and then select Configure, or double-click the device.

2. Select GGSN Access Point CAC Configuration from the Category drop-down box.

The following information appears:

> Access Point Identifier (cgprsAccPtIndex)

> CAC Policy Name (cgprsAccPtCacPolicyName)

> Upstream Bandwidth Pool (cgprsAccPtCacUpStrBandWidthPool)

> Downstream Bandwidth Pool (cgprsAccPtCacDnStrBandWidthPool)

### Access Point Identifier (cgprsAccPtIndex)

Locally unique identifier for this access point on the Gateway GPRS support node (GGSN).

### CAC Policy Name (cgprsAccPtCacPolicyName)

Local policy name that will be used by Call Admission Control (CAC) for the Packet Data Protocol (PDP) contexts associated with this Access Point Name (APN). A zero-length string indicates that no policy is configured.

### Upstream Bandwidth Pool (cgprsAccPtCacUpStrBandWidthPool)

Name of the bandwidth pool used for upstream traffic. A zero-length string indicates that no policy is configured.

A bandwidth pool is a user-defined pool that provides bandwidth pre-allocation details like the amount of available bandwidth and the percentage of bandwidth available to a specific traffic class. CAC uses this information during PDP context activation and modification procedures.

### Downstream Bandwidth Pool (cgprsAccPtCacDnStrBandWidthPool)

Name of the bandwidth pool used for downstream traffic. A zero-length string indicates that no policy is configured.