# Mobile Router System and Mobile Agent Registration Configs

1. ## Right-click on the MWAM Card and select Configure.

2. ## Select category MWAM module.

3. ## Select a row and click the Configure button.

4. ## Select category Mobile Router System and Mobile Agent Registration Configs.

The following information appears:

> Reverse Tunneling Status (cmiMrReverseTunnel)

> Redundancy Group Name (cmiMrRedundancyGroup)

> Max Registration Received Date (cmiMaRegDateMaxRegsReceived)

> Advertisement Flags (cmiMnAdvFlags)

### Reverse Tunneling Status (cmiMrReverseTunnel)

Specifies whether reverse tunneling is enabled on the mobile router or not.

### Redundancy Group Name (cmiMrRedundancyGroup)

Name of the redundancy group used to provide network availability for the mobile router.

### Max Registration Received Date (cmiMaRegDateMaxRegsReceived)

The time at which the maximum number of registration requests in a minute were received by the mobility agent.

### Advertisement Flags (cmiMnAdvFlags)

Flags contained in the 7th byte in the extension of the most recently received mobility agent advertisement:

reverseTunnel | Agent supports reverse tunneling
gre | Agent offers Generic Routing Encapsulation
minEnc | Agent offers Minimal Encapsulation
foreignAgent | Agent is a Foreign Agent
homeAgent | Agent is a Home Agent
busy | Foreign Agent is busy
regRequired | FA registration is required

###