# IPV6 Access Point Statistics 1

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.
2. Select MWAM module from the Category drop-down box.
3. With a device selected in the MWAM module dialog box, click Statistics.
4. Select GGSN Access Point Statistics from the Category drop-down box.
5. With a table entry selected, click Monitor.
6. Select IPV6 Access Point Statistics1 from the Category drop-down box.

The following information appears:

> MS initiated PDPs (cgprsAccPtIpv6MsActivatedPdps)

> Completed MS PDPs (cgprsAccPtIpv6MsSuccActivatedPdps)

> N/W initiated PDPs (cgprsAccPtIpv6NetworkInitDeactPdps)

> Completed N/W PDPs (cgprsAccPtIpv6NetworkInitDeactSuccPdps)

> Dynamic PDPs initiated (cgprsAccPtIpv6MsActivatedDynPdps)

> Dynamic PDPs Completed (cgprsAccPtIpv6MsSuccActivatedDynPdps)

> MS Deactivation PDPs (cgprsAccPtIpv6MsDeactivatedPdps)

### MS initiated PDPs (cgprsAccPtIpv6MsActivatedPdps)

Total number of IPv6 Packet Data Protocol (PDP) context activation procedures initiated by any mobile station (MS) on this access point name (APN).

This object is incremented each time a PDP context creation request is received.

### Completed MS PDPs (cgprsAccPtIpv6MsSuccActivatedPdps)

Total number of successfully completed IPv6 PDP context activation procedures initiated by any MS on this APN.

This object is incremented each time a PDP context creation response message is sent by the gateway GPRS support node (GGSN).

### N/W initiated PDPs (cgprsAccPtIpv6NetworkInitDeactPdps)

Total number of IPv6 PDP context deactivation procedures initiated by the network.

This object is incremented each time the network generates a PDP context deletion request.

### Completed N/W PDPs (cgprsAccPtIpv6NetworkInitDeactSuccPdps)

Total number of successfully completed IPv6 PDP context deactivation procedures initiated by the network on this APN.

This object is incremented each time the GGSN generates a PDP context deletion response message.

### Dynamic PDPs initiated (cgprsAccPtIpv6MsActivatedDynPdps)

Total number of dynamic IPv6 PDP context activation procedures initiated by any MS on this APN. When an MS requests a dynamic PDP address from the public land mobile network (PLMN), a dynamic PDP context activation procedure is initiated.

This object is incremented each time the GGSN receives a PDP context creation request from an MS.

### Dynamic PDPs Completed (cgprsAccPtIpv6MsSuccActivatedDynPdps)

Total number of successfully completed dynamic IPv6 PDP context activation procedures initiated by any MS on this APN.

This object is incremented each time a PDP context creation response message is received.

### MS Deactivation PDPs (cgprsAccPtIpv6MsDeactivatedPdps)

Total number of IPv6 PDP context deactivation procedures initiated by any MS on this APN.