# MIP Security Associations Table

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Configure.

3. Select MIP Security Associations Table.

The following information is displayed:

> Peer Entity's Ip Address (mipSecPeerAddress)

> Security Parameter Index (mipSecSPI)

> Security Algorithm (mipSecAlgorithmType)

> Security Mode (mipSecAlgorithmMode)

> Replay-Protection Method (mipSecReplayMethod)

### Peer Entity's Ip Address (mipSecPeerAddress)

IP address of the peer entity with which the node shares the mobility security association.

### Security Parameter Index (mipSecSPI)

4-byte opaque index within the mobility security association which specifies the security parameters to be used when authenticating the peer.

### Security Algorithm (mipSecAlgorithmType)

Type of security algorithm. There are two possible values:

> other (1)

> md5 (2)

### Security Mode (mipSecAlgorithmMode)

Security mode used by the algorithm. There are two possible values:

> other (1)

> prefixSuffix (2)

### Replay-Protection Method (mipSecReplayMethod)

Replay-protection method supported by the selected security parameter index within the mobility security association.