# Default Gateways

Device>Configure>Default Gateways

Displays information for up to three entries of default gateways.

Address: (mdgGatewayAddr)

The IP address of a default gateway

Type: (mdgGatewayType)

The type of gateway entry; invalid(1): remove this entry; primary(2): the primary entry; other(3): a lower priority entry.

The primary entry will be used first, if it is reachable. Otherwise, one of the other entries will be used. Setting one entry to primary(2) causes any previous primary entry to change to other(3).

Click Create to enter a new gateway IP address and type, and click Apply to make your entry take effect.

Click Delete to remove a selected gateway entry from the table.

Click Cancel to close the dialog box without making any changes. Click Print to print the contents of the dialog box.