# GGSN Charging Tariff Details

From this dialog box, you can view the entry details for tariff times.

Note: This dialog box is available only if the value of cGtpGSNService is set to ggsn.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select GGSN Charging Tariff Details from the Category drop-down box.

The following information is displayed:

> Charging Tariff Time ID (cgprsCgTariffTimeIndex)

> Status of Row (cgprsCgTariffTimeRowStatus)

> Tariff Time in Hours (cgprsCgTariffTimeHour)

> Tariff Time in Minutes (cgprsCgTariffTimeMin)

> Tariff Time in Seconds (cgprsCgTariffTimeSec)

### Charging Tariff Time Identifier (cgprsCgTariffTimeIndex)

Arbitrary nonzero integer value that uniquely identifies each charging tariff time.

### Status of Row (cgprsCgTariffTimeRowStatus)

Status of the row in the tariff time table. Used to create a new row or delete an existing row in the table.

You cannot modify the rows in the table if the value of this object is active. Row Status options notInService and createAndWait are not supported for this object.

### Tariff Time in Hours (cgprsCgTariffTimeHour)

Number of hours as given by the hours part of GPRS tariff time.

### Tariff Time in Minutes (cgprsCgTariffTimeMin)

Number of minutes as given by the minutes part of GPRS tariff time.

### Tariff Time in Seconds (cgprsCgTariffTimeSec)

Number of seconds as given by the seconds part of GPRS tariff time.