# CDMA PDSN PPP Setup Stats Contd

1. Right-click on the MWAM Card and select Configure.
2. Select category MWAM module.
3. Select a row and click the Statistics button.
4. Select category CDMA PDSN PPP Setup Stats Contd.
5. Select a row and click on Monitor.

The following information appears:

> LCP Negotiation Failures (cCdmaPppLcpOptionIssueFailures)

> IPCP Negotiation Failures (cCdmaPppIpcpOptionIssueFailures)

> Authentication Stage Failures (cCdmaPppAuthMaxRetransFailures)

> Successfully LCP Stage Conn (cCdmaPppLcpSuccesses)

> Successful Conn in IPCP Stage (cCdmaPppIpcpSuccesses)

> Successful Conn in Authentication Stage (cCdmaPppAuthSuccesses)

### LCP Negotiation Failures (cCdmaPppLcpOptionIssueFailures)

Total number of PPP connections terminated due to Link Control Protocol (LCP) options negotiation failure such as call back user not negotiating the call back option.

### IPCP Negotiation Failures (cCdmaPppIpcpOptionIssueFailures)

Total number of PPP connections terminated due to Internet Protocol Control Protocol (IPCP) options negotiation failure, such as IP address negotiation.

### Authentication Stage Failures (cCdmaPppAuthMaxRetransFailures)

Total number of PPP connection requests that failed at the authentication stage after the maximum number of retransmissions since the system was last restarted.

### Successfully LCP Stage Conn (cCdmaPppLcpSuccesses)

Total number of PPP connections that entered the LCP stage successfully.

### Successful Conn in IPCP Stage (cCdmaPppIpcpSuccesses)

Total number of PPP connections that entered the IPCP stage successfully.

### Successful Conn in Authentication Stage (cCdmaPppAuthSuccesses)

Total number of PPP connections that succeeded authentication.