# CDMA PDSN PPP Miscellaneous Stats Contd

## Navigation

1. Right-click the device, and select Monitor. The Monitor Device dialog box appears.

2. Select CDMA PDSN PPP Miscellaneous Stats Contd from the Category list.

The following information appears:

> Compression Negotiation Failure (cCdmaPppCompressNegoFailures)

> LCP Echo Requests Transmitted (cCdmaPppTransmittedEchoReqs)

> LCP Echo Requests Retransmitted (cCdmaPppRetransmittedEchoReqs)

> LCP Echo Reply Received (cCdmaPppReceivedEchoReplies)

> LCP Echo Requests Timed Out (cCdmaPppEchoRequestTimeouts)

> Unidentified Protocol Packets Discarded (cCdmaPppUnknownProtocolPktDiscards)

> Bad Length Packets Discarded (cCdmaPppBadLengthPktDiscards)

### Compression Negotiation Failure (cCdmaPppCompressNegoFailures)

The total number of PPP negotiations that failed due to compression negotiation failure since the system was last restarted.

### LCP Echo Requests Transmitted (cCdmaPppTransmittedEchoReqs)

The total number of LCP Echo requests transmitted since the system was last restarted.

### LCP Echo Requests Retransmitted (cCdmaPppRetransmittedEchoReqs)

The total number of LCP Echo requests retransmitted since the system was last restarted.

### LCP Echo Reply Received (cCdmaPppReceivedEchoReplies)

The total number of LCP Echo replies received since the system was last restarted.

### LCP Echo Requests Timed Out (cCdmaPppEchoRequestTimeouts)

The total number of LCP Echo requests timed out since the system was last restarted.

### Unidentified Protocol Packets Discarded (cCdmaPppUnknownProtocolPktDiscards)

The total number of packets discarded at PPP stack due to protocol value not being identified, since the system was last restarted.

### Bad Length Packets Discarded (cCdmaPppBadLengthPktDiscards)

The total number of PPP packets discarded stack due to bad length, since the system was last restarted.