# Content Switching Module - Create CSM VLANs

The Create CSM VLAN dialog box is used to create VLANs associated with the content switching module.

## Navigation

1. Right-click the blade, then select CSM Configuration....

2. Click Create.

The following information appears:

VLAN ID

VLAN Type

IP Address

Subnet Mask

Gateway

### VLAN ID

Number assigned to a particular VLAN.

### VLAN Type

Type of VLAN. Type shows if the VLAN resides on a client or a server.

### IP Address

IP address associated with a particular VLAN.

### Subnet Mask

IP mask address associated with a particular VLAN.

### Gateway

IP gateway for the traffic in a particular VLAN.