# Cross Bar Module Status

Device>Configure>Cross Bar Module Status

This dialog box provides information on fabric modules.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- Crossbar Fabric Active Slot

- Crossbar Fabric Backup Slot

- Minimum Fabric Modules

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to make changes take effect.

- Click Cancel to close the dialog box.

- Click Refresh to reload the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access the online help.

Crossbar Fabric Active Slot (cc6kxbarFabricActiveSlot)

Indicates the slot number of the active switching fabric module. A value of zero indicates that the active switching fabric module is either powered down or not present in the chassis.

Crossbar Fabric Backup Slot (cc6kxbarFabricBackupSlot)

Indicates the slot number of the backup switching fabric module. A value of zero indicates that the backup switching fabric module is either powered down or not present in the chassis.

Minimum Fabric Modules (cc6kxbarMinFabricPresent)

Object cc6kxbarMinFabricPresent indicates the minimum number of switching fabric capable modules present in the system for any switching fabric capable module in 'crossbarmode' (which is indicated by cc6kxbarModuleModeSwitchingMode when cc6kxbarTruncatedModeAllowed is set to 'true').

When cc6kxbarMinFabricPresent has a value larger than the number of slots in the system, then the value of cc6kxbarTruncatedModeAllowed has no effect.