# IGMP Snooping Capable Interfaces Tx Statistics

To launch the IGMP Snooping Capable Interfaces Tx Statistics dialog box:

1. Select Device > Monitor > IGMP Snooping Statistics.

2. With an interface selected, click Monitor.

This dialog box provides Tx statistics for IGMP Snooping capable interfaces.

The following data is displayed:

- General Queries Transmitted (cisTxGeneralQueries)

- Group Specific Queries Transmitted (cisTxGroupSpecificQueries)

- Total Membership Reports Transmitted (cisTxReports)

- Total Membership Leaves Transmitted (cisTxLeaves)

The following list specifies buttons in this dialog box, as well as their function:

- To specify the refresh rate for this dialog box, select a value from the drop-down box.

- Click Start/Stop to begin/end device monitoring.

> Note: The Start/Stop toggle feature is supported only by CiscoView 5.x.

- Click Cancel to close the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

General Queries Transmitted (cisTxGeneralQueries)

Number of general queries that have been transmitted through an interface.

Group Specific Queries Transmitted (cisTxGroupSpecificQueries)

Total number of group-specific queries that have been transmitted through an interface.

Total Membership Reports Transmitted (cisTxReports)

Total number of membership reports that have been transmitted through an interface.

Total Membership Leaves Transmitted (cisTxLeaves)

Total number of leave messages that have been transmitted through an interface.