# SRP Higher Layer Errors

Use this option to monitor higher layer error statistics traffic reception for the current interval of a particular side of a particular SRP interface.

## Procedure

> 1. Right-click the SRP interface and select Monitor from the popup menu.

> The Monitor Port dialog box appears.

> 2. Select Error Statistics - Current Interval from the Category menu.

> The Error Statistics - Current Interval dialog box appears.

3. Select Interface Side.

4. Click Monitor button.

5. Select Higher Layer Errors from the Category menu.

The Error Statistics - Current Interval dialog box for that particular side displays the following higher layer error information:

Discarded Packets (srpErrCntCurrHostRxDiscardPkts)

Short Packets (srpErrCntCurrHostRxShortPkts)

Giant Packets (srpErrCntCurrHostRxGiantPkts)

## Related Topics

SRP Physical Layer Errors

### Discarded Packets (srpErrCntCurrHostRxDiscardPkts)

Number of packets that cannot be delivered to the higher layer due to resource limitation, during a 15 minute interval.

### Short Packets (srpErrCntCurrHostRxShortPkts)

Number of packets that cannot be delivered to the higher layer for being too short, during a 15 minute interval.

### Giant Packets (srpErrCntCurrHostRxGiantPkts)

Number of packets that cannot be delivered to the higher layer for being too big, during a 15 minute interval.