# GGSN APN Aggregate Routes

The GGSN APN Aggregate Routes category of the Chassis Configuration dialog box lists the APN details including aggregation.

Note This dialog can be viewed if cGtpGSNService is set to 'ggsn'

## Procedure

1. Right-click the device and then select Configure, or double-click the device.

2. Select GGSN APN Aggregate Routes from the Category list.

The following information appears:

Internet Address Type (cgprsAccPtAggregIpAddrType)

IP Address (cgprsAccPtAggregIpAddr)

Net Mask (cgprsAccPtAggregIpMask)

Row Status (cgprsAccPtAggregRowStatus)

### Internet Address Type (cgprsAccPtAggregIpAddrType)

Type of Internet address denoted by cgprsAccPtAggregIpAddr.

### IP Address (cgprsAccPtAggregIpAddr)

IP address whose network prefix is defined by cgprsAccPtAggregIpMask.

When this object is set cgprsAccPtAggregIpMask must be specified.

### Net Mask (cgprsAccPtAggregIpMask)

Net-mask pertaining to cgprsAccPtAggregIpAddr.

### Row Status (cgprsAccPtAggregRowStatus)

Status of the row in the aggregate route table. Used to create a new row or delete an existing row in the table.

To create a row set the object to createAndGo.

To delete a row set the object to destroy.