# MIP Security Violations Table

The table displays the following information:

Violator's IpAddress (mipSecViolatorAddress)

Security Violations Count (mipSecViolationCounter)

Latest Security Violation's SPI (mipSecRecentViolationSPI)

Latest Security Violation's Time(mipSecRecentViolationTime )

Latest Security Violation's 4 LSBs(mipSecRecentViolationIDLow )

Latest Security Violation's 4 MSBs (mipSecRecentViolationIDHigh)

Latest Security Violation's Reason (mipSecRecentViolationReason)

### Violator's IpAddress (mipSecViolatorAddress)

Violator's IP address.

### Security Violations Count (mipSecViolationCounter)

Total number of security violations for the peer.

### Latest Security Violation's SPI (mipSecRecentViolationSPI)

SPI of the most recent security violation for the peer.

If the security violation is due to an identification mismatch, then this is the SPI from the Mobile-Home Authentication Extension.

If the security violation is due to an invalid authenticator, then this is the SPI from the offending authentication extension.

In all other cases, value is set to zero.

### Latest Security Violation's Time(mipSecRecentViolationTime )

Time of the most recent security violation for the peer.

### Latest Security Violation's 4 LSBs(mipSecRecentViolationIDLow )

Low-order 32 bits of identification used in request or reply of the most recent security violation for the peer.

### Latest Security Violation's 4 MSBs (mipSecRecentViolationIDHigh)

High-order 32 bits of identification used in request or reply of the most recent security violation for the peer.

### Latest Security Violation's Reason (mipSecRecentViolationReason)

Reason for the most recent security violation for the peer.

Possible values are:

noMobilitySecurityAssociation (1)

badAuthenticator (2)

badIdentifier (3)

badSPI (4)

missingSecurityExtension (5)

other (6)