# CDMA PDSN Service Option Table

This dialog box is applicable to Member and Peer to Peer clusters.

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Configure.

3. Select CDMA PDSN Service Option Table.

The following information is displayed:

> Service Option (cCdmaServiceOptionIndex)

> Rp Session Success (cCdmaServiceOptionSucesses)

> Rp Session Failure (cCdmaServiceOptionFailures)

### Service Option (cCdmaServiceOptionIndex)

Service option, as defined by IOS 4.1. A service option is used to uniquely index table entries. Service options (as defined in 3GPP2 4.1) are:

Value | Description
6 | smsRate1
9 | loopback13K
12 | asyncDataRate2
13 | group3FaxRate2
14 | smsRate2
15 | packetData144k
18 | otapaRate1
19 | otapaRate2
22 | packetDataRs1fRs1r
23 | packetDataRs1fRs2r
24 | packetDataRs2fRs1r
25 | packetDataRs2fRs2
32 | is2000TestData
33 | packetData3G
37 | isdn64k
54 | is2000Markov
55 | is2000Loopback
4103 | packetDataRev1

### Rp Session Success (cCdmaServiceOptionSucesses)

Number of times the device succeeded in setting up a radio packet (RP) session for a particular service option defined by IOS 4.1.

### Rp Session Failure (cCdmaServiceOptionFailures)

Number of times the device failed in setting up a RP session for a particular service option defined by IOS 4.1.