# GGSN Aggregate Routes Table

The GGSN Aggregate Routes Table category of the Chassis Configuration dialog box displays details of the aggregate routes table.

Note This dialog can be viewed if cGtpGSNService is set to 'ggsn'.

## Procedure

1. Right-click the device and then select Configure, or double-click the device.

2. Select GGSN Aggregate Routes Table from the Category list.

The following information appears:

Default Address Type (cGgsnDefaultAggregIpAddrType)

Default IP Address (cGgsnDefaultAggregIpAddr)

Default IP Address Mask (cGgsnDefaultAggregIpMask)

Create/Delete Row (cGgsnDefaultAggregRowStatus)

### Default Address Type (cGgsnDefaultAggregIpAddrType)

Type of Internet address denoted by cGgsnDefaultAggregIpAddr.

### Default IP Address (cGgsnDefaultAggregIpAddr)

IP address whose network prefix is defined by cGgsnDefaultAggregIpMask.

### Default IP Address Mask (cGgsnDefaultAggregIpMask)

Net mask pertaining to cGgsnDefaultAggregIpAddr.

### Create/Delete Row (cGgsnDefaultAggregRowStatus)

Status of the row in Aggregate Routes Table. This object is used to create a new row or delete an existing row in the table.

To create a row, set this object to createAndGo.

To delete a row, set this object to destroy.

The values createAndWait and notInService are not supported.