# GGSN APN History

The GGSN APN History category of the Chassis Configuration dialog box lists the access point notifications.

Note This dialog can be viewed if cGtpGSNService is set to 'ggsn'

## Procedure

1. Right-click the device and then select Configure, or double-click the device.

2. Select GGSN APN History from the Category list.

The following information appears:

Notification Identifier (cgprsAccPtCfgNotifIndex)

Access Point (cgprsAccPtCfgNotifAccPtIndex)

Notification Reason (cgprsAccPtCfgNotifReason)

### Notification Identifier (cgprsAccPtCfgNotifIndex)

Arbitrary nonzero integer value that uniquely identifies each notification previously sent by the GPRS. The value increases monotonically with each notification sent by the GGSN. When the object reaches the maximum value of 4294967295 wraps to 1.

### Access Point (cgprsAccPtCfgNotifAccPtIndex)

Access point that has been created, changed or modified.

### Notification Reason (cgprsAccPtCfgNotifReason)

Reason for the notification. Reason can be:

modification(1)

creation(2)

deletion(3)