# Monitoring Unusual Token Ring Errors

Select Unusual Token Ring Errors from the CATEGORY box to display the following information in the CiscoView Monitor Port window:

Internal Errors

Frequency Errors

Aborts

Remove Ring Station Requests

Lobe Data Path Errs

Signals Lost

# Internal Errors (dot5StatsInternalErrors)

This counter increments when a station diagnoses an internal error.

# Frequency Errors (dot5StatsFreqErrors)

Indicates the number of times that the frequency of the incoming signal is not within the expected range.

# Aborted Trans (AbortTransErrors)

This counter increments when the station transmits an abort delimiter.

# Remove Ring Station Reqs (dot5StatsRemove)

Indicates the number of times the interface has detected an open or short circuit in the lobe data path.

# Lobe Data Path Errors (dot5StatsLobeErrors)

Shows the number of times the interface has detected an open or short circuit in the lobe data path.

# Signals Lost (dot5StatsSignalLoss)

Indicates the number of times the specified interface detected loss of signal.