Scheduled Reset

# Scheduled Reset

Device > Configure > Scheduled Reset

After selecting and invoking the Scheduled reset menu in the device configuration menu, a dialog window appears in which the user can perform a scheduled reset operation.

Scheduled Reset (resetEnable)

The Disable setting will disable the previously scheduled reset time. The Enable setting will enable the previously scheduled reset time.

Reset Date and Time (csyScheduledResetTime)

The scheduled date and time the switch will be reset at. The maximum scheduled time is 24 days from the current system clock time. Setting this object value to be before the current system clock or beyond the maximum scheduled time limit will be rejected by the system.

After the system has accepted the scheduled reset time, if the system clock is advanced ahead of the scheduled reset time, then reset will occur approximately 5 minutes after the current clock.

Reset Action (csyScheduledResetAction)

Writing reset (1) to this object performs the normal reset operation on the active supervisor module. Writing resetMinDown (2) to this object resets the switch with a minimal system down time at the scheduled time. The resetMinDown is only supported on Switches which have redundant supervisor modules.

The resetMinDown is supported only for switches with redundant supervisor module.

Reset Reason (csyScheduledResetReason)

Indicates the reason for the systems scheduled reset. After the system is reset, this object value will be an empty string.