# SSG Status

The SSG Status category of the Configure dialog box displays details on the service selection gateway (SSG) configuration.

## Procedure

1. Right-click the device, then select Configure, or double-click the device.

2. Select SSG Status from the category list.

The following information appears:

SSG Service State (cssgCfgSsgEnabled)

AutoDomain Status (cssgCfgAutoDomainMode)

Local Forwarding Status (cssgCfgLocalForwardingEnabled)

Auto Logoff Status (cssgCfgAutoLogOffMode)

Radius Proxy Status (cssgCfgRadiusProxyEnabled)

TCP Redirect Status (cssgCfgTcpRedirectEnabled)

NAT Status (cssgCfgAutoDomainNatEnabled)

PortBundle-Host Status (cssgCfgPortBundleHostKeyEnabled)

Transparent Pass Status (cssgCfgTransPassThroughEnabled)

Accounting Status (cssgCfgAccountingEnabled)

Forwarding State (cssgCfgRadiusFwdAcctPktsEnabled)

Radius Reboot Status (cssgCfgRadiusClntRbtNotifEnabled)

AAA Reboot Status (cssgCfgAAAServerDownNotifEnabled)

Enable TAL(cssgCfgTalEnabled)

### SSG Service State (cssgCfgSsgEnabled)

Indicates whether service selection gateway (SSG) service is enabled.

### AutoDomain Status (cssgCfgAutoDomainMode)

Indicates whether the auto-domain feature is enabled.

The auto-domain feature allows the user to be connected automatically to a service based on the access-point name or structured username.

Auto-domain status can be:

Value | Description
1 | disabled
2 | basic
3 | extended

### Local Forwarding Status (cssgCfgLocalForwardingEnabled)

Indicates whether local forwarding is enabled.

Local forwarding feature allows service selection gateway (SSG) to forward packets locally among connected subscribers.

### Auto Logoff Status (cssgCfgAutoLogOffMode)

Indicates whether the auto-logoff feature is enabled.

The auto-logoff feature allows service selection gateway (SSG) to initiate logoff if connectivity to a host is lost. Connectivity to a host is checked using address resolution protocol or Internet control message protocol.

### Radius Proxy Status (cssgCfgRadiusProxyEnabled)

Indicates whether RADIUS proxy feature is enabled.

The remote authentication dial-in user service (RADIUS) proxy feature allows service selection gateway (SSG) to act as a generic RADIUS-proxy for non-service-selection dashboard clients such as gateway GPRS selection node.

### TCP Redirect Status (cssgCfgTcpRedirectEnabled)

Indicates whether TCP redirect is enabled.

TCP redirect feature redirects certain TCP packets to captive portals.

### NAT Status (cssgCfgAutoDomainNatEnabled)

Indicates whether network address translation is available for auto-domain users.

The network address translation feature determines whether the auto-domain service gets the IP address assigned by the auto-domain service.

### PortBundle-Host Status (cssgCfgPortBundleHostKeyEnabled)

Indicates whether port bundle-host key feature is enabled.

The port bundle-host key feature allows subscriber edge service manager to identify subscribers based on the PortBundle (combination of IP address and a range of ports) assigned by service selection gateway (SSG).

### Transparent Pass Status (cssgCfgTransPassThroughEnabled)

Indicates whether the transparent pass through feature is enabled.

The transparent pass through feature allows unauthenticated subscriber traffic to be routed through SSG in either direction.

### Accounting Status (cssgCfgAccountingEnabled)

Indicates whether accounting is enabled.

The accounting feature allows service selection gateway (SSG) to generate accounting records and send them to the authentication, authorization and accounting (AAA) server.

### Forwarding State (cssgCfgRadiusFwdAcctPktsEnabled)

Indicates whether service selection gateway (SSG) forwards accounting packets received from radius clients to the AAA server.

### Radius Reboot Status (cssgCfgRadiusClntRbtNotifEnabled)

Indicates whether service selection gateway (SSG) generates a notification if a client of the RADIUS reboots.

### AAA Reboot Status (cssgCfgAAAServerDownNotifEnabled)

Indicates whether service selection gateway (SSG) generates a notification if connectivity to an AAA server goes down or is lost.

### Enable TAL(cssgCfgTalEnabled)

An indication of whether Transparent Auto Logon feature is enabled on SSG.