# RP Registration Request Statistics

1. Right-click on the MWAM Card and select Configure.
2. Select category MWAM module.
3. Select a row and click the Statistics button.
4. Select category CDMA PDSN PCF & SO Based Statistics.
5. Select a row and click the RP Registration Statistics button and from the category select RP Registration Request Statistics.

The following information appears:

> Initial A11 Registration Requests (cCdmaPcfSoRpInitRegRcvdReqs)

> A11 Re-registration Request (cCdmaPcfSoRpReRegRcvdReqs)

> A11 De-registration Request (cCdmaPcfSoRpDeRegRcvdReqs)

> Handoff Registration Request (cCdmaPcfSoRpHandoffRegRcvdReqs)

> Airlink Start Re-registration Request (cCdmaPcfSoRpReRegAirlinkStarts)

> Airlink Stop Re-registration Request (cCdmaPcfSoRpReRegAirlinkStops)

> Airlink Stop De-registration Request (cCdmaPcfSoRpDeRegAirlinkStops)

### Initial A11 Registration Requests (cCdmaPcfSoRpInitRegRcvdReqs)

Number of Initial A11 Registration requests received since the system was last restarted.

### A11 Re-registration Request (cCdmaPcfSoRpReRegRcvdReqs)

Number of A11 Re-Registration requests received since the system was last restarted.

### A11 De-registration Request (cCdmaPcfSoRpDeRegRcvdReqs)

Number of A11 De-Registration requests received since the system was last restarted.

### Handoff Registration Request (cCdmaPcfSoRpHandoffRegRcvdReqs)

Number of A11 Handoff Registration requests received since the system was last restarted.

### Airlink Start Re-registration Request (cCdmaPcfSoRpReRegAirlinkStarts)

Number of A11 Re-Registration requests containing Airlink Start since the system was last restarted.

### Airlink Stop Re-registration Request (cCdmaPcfSoRpReRegAirlinkStops)

Number of A11 Re-Registration requests containing Airlink Stop since the system was last restarted.

### Airlink Stop De-registration Request (cCdmaPcfSoRpDeRegAirlinkStops)

Number of A11 De-Registration requests containing Airlink Stop since the system was last restarted.