# Token Ring Port Configuration Information

The configure port window displays the following information for a token ring port:

> Index (dot5IfIndex)

> Command (dot5Commands)

> Error Report (dot5RingStatus)

> Open/Close Info (dot5RingStatus)

> Result of Last Enter Ring (dot5RingOpenStatus)

> Speed (dot5RingSpeed)

> Upstream Neighbor MAC Address (dot5RingUpStream)

Index (dot5IfIndex)

Specifies the ifIndex value from the MIB interface table for this interface.

Command (dot5Commands)

Name of a command variable used to request a state change. Possible values are no-op, open, reset, and close.

Open means join the ring; close means leave.

Error Report (dot5RingStatus)

Number of errors on the specified port.

Open/Close Info (dot5RingStatus)

Provides information related to entering/leaving the ring.

Result of Last Enter Ring (dot5RingOpenStatus)

Indicates whether the last attempt to enter the ring was successful, and if not, shows the reason for the failure.

Speed (dot5RingSpeed)

Indicates the bandwidth for the ring. Possible values are 1 Mbps, 4 Mbps, 16 Mbps, and unknown. A read-only variable.

Upstream Neighbor MAC Address (dot5RingUpStream)

Specifies the MAC address of the upstream neighbor.