# SRP Higher Layer Interval Statistics

Use this option to monitor higher layer interval statistics of a particular interface.

## Procedure

To access higher layer interval statistics information:

1. Right-click the port and select SRP Interface Statistics from the popup menu.

Higher Layer Interval Statistics dialog box appears.

3. Select Higher Layer Interval Statistics from the Category menu to display higher layer interval statistics information.

Higher Layer Interval Statistics dialog box displays:

Interface Side (srpHostIntInterfaceSide)

Interval Number (srpHostIntNumber)

### Interface Side (srpHostIntInterfaceSide)

Interface side containing row information.

### Interval Number (srpHostIntNumber)

A number between 1 and 96, which identifies the interval for available statistics.

1 means interval is the most recent completed 15 minute interval.

N means interval precedes N-1.

## Related Topics

The CiscoView Monitor Window

Monitoring Ports

Monitoring the Device

Monitoring the Device Environment

Monitoring Devices and Components