# Home Agent Redundancy Statistics - Binding Updates

## Navigation

1. Right-click the device, and select Monitor. The Monitor Device dialog box appears.

2. Select Home Agent Redundancy Statistics-Binding Updates from the Category list.

The following information appears:

> Binding Updates (cmiHaRedunSentBUs)

> Binding Updates-No Ack (cmiHaRedunFailedBUs)

> Ack Received (cmiHaRedunReceivedBUAcks)

> Total Updates Sent (cmiHaRedunTotalSentBUs)

> Bindings Received (cmiHaRedunReceivedBUs)

> Ack Sent (cmiHaRedunSentBUAcks)

> Requests Sent (cmiHaRedunSentBIReqs)

> Failed Requests (cmiHaRedunFailedBIReqs)

> Total Requests (cmiHaRedunTotalSentBIReqs)

### Binding Updates (cmiHaRedunSentBUs)

The total number of binding updates sent by the home agent.

### Binding Updates-No Ack (cmiHaRedunFailedBUs)

The total number of binding updates sent by the home agent for which no acknowledgement is received from the standby home agent.

### Ack Received (cmiHaRedunReceivedBUAcks)

The total number of acknowledgements received in response to binding updates sent by the home agent.

### Total Updates Sent (cmiHaRedunTotalSentBUs)

The total number of binding updates sent by the home agent including retransmissions of the same binding update.

### Bindings Received (cmiHaRedunReceivedBUs)

The total number of binding updates received by the home agent.

### Ack Sent (cmiHaRedunSentBUAcks)

The total number of acknowledgements sent in response to binding updates received by the home agent.

### Requests Sent (cmiHaRedunSentBIReqs)

The total number of binding information requests sent by the home agent.

### Failed Requests (cmiHaRedunFailedBIReqs)

The total number of binding information requests sent by the home agent for which no reply is received from the active home agent.

### Total Requests (cmiHaRedunTotalSentBIReqs)

The total number of binding information requests sent by the home agent for which no reply is received from the active home agent.