# RP Update Registration Failures Contd

1. Right click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Statistics button.

4. Select category CDMA PDSN PCF & SO Based Statistics.

5. Select a row and click on the RP Update Statistics button and from the Category select RP Update Registration Failures Contd.

The following information appears:

> Unspecified Reasons (cCdmaSoRpUpdHandoffReaUnSpecFails)

> Administrative Prohibition (cCdmaSoRpUpdHandoffAdmProhibFails)

> MN Authentication (cCdmaSoRpUpdHandoffMNAuthenFails)

> Registration Identity Mismatch (cCdmaSoRpUpdHandoffIdMismatchFails)

> Poorly Formed Request (cCdmaSoRpUpdHandoffBadReqFails)

### Unspecified Reasons (cCdmaSoRpUpdHandoffReaUnSpecFails)

Number of update registrations that failed for an unspecified reason since the system was last restarted. The update is sent as a result of inter PCF handoff.

### Administrative Prohibition (cCdmaSoRpUpdHandoffAdmProhibFails)

### Number of update registrations that failed due to administrative prohibition since the system was last restarted. The update is sent as a result of inter PCF handoff.

### MN Authentication (cCdmaSoRpUpdHandoffMNAuthenFails)

Number of update registrations that failed due to mobile node authentication failure since the system was last restarted. The update is sent as a result of inter PCF handoff.

### Registration Identity Mismatch (cCdmaSoRpUpdHandoffIdMismatchFails)

Number of registrations that failed due to registration identity mismatch since the system was last restarted. The update is sent as a result of inter PCF handoff.

### Poorly Formed Request (cCdmaSoRpUpdHandoffBadReqFails)

Number of update registrations failed due to poorly formed request since the system was last restarted. The update is sent as a result of inter PCF handoff.