# SSG Status

The SSG Status dialog box displays details on the current Service Selection Gateway (SSG) configuration.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select SSG Status from the Category list.

The following information is displayed:

> SSG Service State (cssgCfgSsgEnabled)

> AutoDomain Status (cssgCfgAutoDomainMode)

> Local Forwarding Status (cssgCfgLocalForwardingEnabled)

> Auto Logoff Status (cssgCfgAutoLogOffMode)

> Radius Proxy Status (cssgCfgRadiusProxyEnabled)

> TCP Redirect Status (cssgCfgTcpRedirectEnabled)

> NAT Status (cssgCfgAutoDomainNatEnabled)

> PortBundle-Host Status (cssgCfgPortBundleHostKeyEnabled)

> Transparent Pass Status (cssgCfgTransPassThroughEnabled)

> Accounting Status (cssgCfgAccountingEnabled)

> Forwarding State (cssgCfgRadiusFwdAcctPktsEnabled)

> Radius Reboot Status (cssgCfgRadiusClntRbtNotifEnabled)

> AAA Reboot Status (cssgCfgAAAServerDownNotifEnabled)

> Enable TAL (cssgCfgTalEnabled)

### SSG Service State (cssgCfgSsgEnabled)

Indicates whether SSG service is enabled.

### AutoDomain Status (cssgCfgAutoDomainMode)

Indicates whether the auto-domain feature is enabled. This feature allows the user to be connected automatically to a service based on the access-point name or structured username.

Auto-domain status can be one of three values:

Value | Description
1 | disabled
2 | basic
3 | extended

### Local Forwarding Status (cssgCfgLocalForwardingEnabled)

Indicates whether local forwarding is enabled.

Local forwarding feature allows SSG to forward packets locally among connected subscribers.

### Auto Logoff Status (cssgCfgAutoLogOffMode)

Indicates whether the auto-logoff feature is enabled.

The auto-logoff feature allows SSG to initiate logoff if connectivity to a host is lost. Connectivity to a host is checked using either the Address Resolution Protocol (ARP) or Internet Control Message Protocol (ICMP). There are three possible values:

> disabled(1)

> icmp(2)

> arp(3)

### Radius Proxy Status (cssgCfgRadiusProxyEnabled)

Indicates whether RADIUS proxy feature is enabled.

The remote authentication dial-in user service (RADIUS) proxy feature allows SSG to act as a generic RADIUS-proxy for non-service-selection dashboard clients such as gateway GPRS selection node.

### TCP Redirect Status (cssgCfgTcpRedirectEnabled)

Indicates whether TCP redirect is enabled.

TCP redirect feature redirects certain TCP packets to captive portals.

### NAT Status (cssgCfgAutoDomainNatEnabled)

Indicates whether network address translation is available for auto-domain users.

The network address translation feature determines whether the auto-domain service gets the IP address assigned by the auto-domain service.

### PortBundle-Host Status (cssgCfgPortBundleHostKeyEnabled)

Indicates whether port bundle-host key feature is enabled.

The port bundle-host key feature allows subscriber edge service manager to identify subscribers based on the PortBundle (combination of IP address and a range of ports) assigned by SSG.

### Transparent Pass Status (cssgCfgTransPassThroughEnabled)

Indicates whether the transparent pass through feature is enabled.

The transparent pass through feature allows unauthenticated subscriber traffic to be routed through SSG in either direction.

### Accounting Status (cssgCfgAccountingEnabled)

Indicates whether accounting is enabled.

The accounting feature allows SSG to generate accounting records and send them to the authentication, authorization and accounting (AAA) server.

### Forwarding State (cssgCfgRadiusFwdAcctPktsEnabled)

Indicates whether SSG forwards accounting packets received from radius clients to the AAA server.

### Radius Reboot Status (cssgCfgRadiusClntRbtNotifEnabled)

Indicates whether SSG generates a notification if a client of the RADIUS reboots.

### AAA Reboot Status (cssgCfgAAAServerDownNotifEnabled)

Indicates whether SSG generates a notification if connectivity to an AAA server goes down or is lost.

### Enable TAL (cssgCfgTalEnabled)

An indication of whether Transparent Auto Logon feature is enabled on SSG.

Note: This is available from SSG 1.2.