# Monitoring SONET Line Current Statistics

Select SONET Line Current Statistics from the Monitor pull-down menu to monitor SONET line statistics collected for the current 15 minute interval. The following values are displayed:

Errored Seconds (sonetLineCurrentESs)

Severely Errored Seconds (sonetLineCurrentSESs)

Code Violation (sonetLineCurrentCVs)

Unavailable Seconds (sonetLineCurrentUASs)

### Errored Secs (sonetLineCurrentESs)

The number of seconds during the current 15 minute interval that a line error occurred.

### Severely Errored Secs (sonetLineCurrentSESs)

The number of seconds during the current 15 minute interval that a severe error occurred for this line.

### Code Violation (sonetLineCurrentCVs)

The number of seconds during the current 15 minute interval that a coding violation occurred for this line.

### Unavailable Seconds (sonetLineCurrentUASs)

The number of seconds during the current 15 minute interval that the line was not available.