# SRP Physical Layer Errors

Use this option to view layer 1 physical medium traffic reception for a particular interval of a particular side of a particular SRP interface.

## Procedure

> 1. Right-click the SRP interface and select Configure from the popup menu.

> The Configure Port dialog box appears.

> 2. Select SRP Error Statistics - History from the Category menu.

> The SRP Error Statistics - History dialog box appears.

3. Select an Interval.

4. Click the Statistics button.

5. Select Physical Layer Errors from the Category menu.

The SRP Error Statistics - History dialog box displays the following physical layer error information:

TTL Exp. Packet Discard (srpErrCntIntRingRxTtlExpPkts)

Short Packets (srpErrCntIntRingRxShortPkts)

Giant Packets (srpErrCntIntRingRxGiantPkts)

Aborted Packets (srpErrCntIntRingRxAbortPkts)

CRC Error Packets (srpErrCntIntRingRxCRC)

## Related Topics

SRP Higher Layer Errors

### TTL Exp. Packet Discard (srpErrCntIntRingRxTtlExpPkts)

Number of expired packets, received from layer 1 physical medium during a 15 minute interval in the past 24 hours.

### Short Packets (srpErrCntIntRingRxShortPkts)

Number of short packets, received from layer 1 physical medium during a 15 minute interval in the past 24 hours.

### Giant Packets (srpErrCntIntRingRxGiantPkts)

Number of giant packets, received from layer 1 physical medium during a 15 minute interval in the past 24 hours.

### Aborted Packets (srpErrCntIntRingRxAbortPkts)

Number of aborted packets, received from layer 1 physical medium during a 15 minute interval in the past 24 hours.

### CRC Error Packets (srpErrCntIntRingRxCRC)

Number of packets with CRC errors, received from layer 1 physical medium during a 15 minute interval in the past 24 hours.