# AHDLC Traffic Details

The AHDLC Traffic Details dialog box allows you to monitor delivery and generation information about the asynchronous high-level data link control (AHDLC) engine traffic.

## Procedure

1. Right-click the device, then select Configure, or double-click the device.

2. Select AHDLC Engine Details from the Category list.

3. Select an AHDLC engine and click Traffic Monitor.

The following information appears:

Active Channels (cCdmaAhdlcEngineChannelsInUse)

Outgoing Octets To Encode (cCdmaAhdlcOutgoingOctetsToEncode)

Outgoing Octets Encoded (cCdmaAhdlcOutgoingOctetsEncoded)

Outgoing Packets To Encode (cCdmaAhdlcOutgoingPktsToEncode)

Outgoing Packets Encoded (cCdmaAhdlcOutgoingPktsEncoded)

Incoming Octets To Decode (cCdmaAhdlcIncomingOctetsToDecode)

Incoming Octets Decoded (cCdmaAhdlcIncomingOctetsDecoded)

Incoming Packets To Decode (cCdmaAhdlcIncomingPktsToDecode)

Incoming Packets Decoded (cCdmaAhdlcIncomingPktsDecoded)

### Active Channels (cCdmaAhdlcEngineChannelsInUse)

Number of active channels handled by the engine.

### Outgoing Octets To Encode (cCdmaAhdlcOutgoingOctetsToEncode)

Total number of outgoing octets delivered to the asynchronous high-level data link control (AHDLC) engine for encoding since system was last restarted.

The counter value could have discontinuities when the management system is reinitialized and at other times as shown by the value of cCdmaAhdlcDiscontinuityTime.

### Outgoing Octets Encoded (cCdmaAhdlcOutgoingOctetsEncoded)

Total number of outgoing octets generated by the asynchronous high-level data link control (AHDLC) engine through AHDLC encoding since system was last restarted.

The counter value could have discontinuities when the management system is reinitialized and at other times as shown by the value of cCdmaAhdlcDiscontinuityTime.

### Outgoing Packets To Encode (cCdmaAhdlcOutgoingPktsToEncode)

Total number of outgoing packets delivered to the asynchronous high-level data link control (AHDLC) engine for AHDLC encoding since system was last restarted.

The counter value could have discontinuities when the management system is reinitialized and at other times as shown by the value of cCdmaAhdlcDiscontinuityTime.

### Outgoing Packets Encoded (cCdmaAhdlcOutgoingPktsEncoded)

Total number of outgoing packets generated by the asynchronous high-level data link control (AHDLC) engine through AHDLC encoding since system was last restarted.

The counter value could have discontinuities when the management system is reinitialized and at other times as shown by the value of cCdmaAhdlcDiscontinuityTime.

### Incoming Octets To Decode (cCdmaAhdlcIncomingOctetsToDecode)

Total number of incoming octets delivered to the asynchronous high-level data link control (AHDLC) engine for AHDLC decoding since system was last restarted.

The counter value could have discontinuities when the management system is reinitialized and at other times as shown by the value of cCdmaAhdlcDiscontinuityTime.

### Incoming Octets Decoded (cCdmaAhdlcIncomingOctetsDecoded)

Total number of incoming octets generated by the asynchronous high-level data link control (AHDLC) engine through AHDLC decoding since system was last restarted.

The counter value could have discontinuities when the management system is reinitialized and at other times as shown by the value of cCdmaAhdlcDiscontinuityTime.

### Incoming Packets To Decode (cCdmaAhdlcIncomingPktsToDecode)

Number of packets dropped by the engine due to insufficient memory during asynchronous high-level data link control (AHDLC) decoding since system was last restarted.

The counter value could have discontinuities when the management system is reinitialized and at other times as shown by the value of cCdmaAhdlcDiscontinuityTime.

### Incoming Packets Decoded (cCdmaAhdlcIncomingPktsDecoded)

Total number of incoming packets generated by the asynchronous high-level data link control (AHDLC) engine through AHDLC decoding since system was last restarted.

The counter value could have discontinuities when the management system is reinitialized and at other times as shown by the value of cCdmaAhdlcDiscontinuityTime.