# GGSN History Table

The GGSN History Table category of the Chassis Configuration dialog box provides details of the GGSN Notification History Table.

Note This dialog can be viewed if cGtpGSNService is set to 'ggsn'

## Procedure

1. Right-click the device and then select Configure, or double-click the device.

2. Select GGSN History Table from the Category list.

The following information appears:

Index (cGgsnHistNotifIndex)

Type of Notification (cGgsnHistNotifType)

Severity Level (cGgsnHistNotifSeverity)

Notification Time (cGgsnHistNotifTimestamp)

Address Reachable (cGgsnHistNotifGgsnIpAddrType)

Device that generated Notification (cGgsnHistNotifGgsnIpAddr)

Additional Type Information (cGgsnHistNotifInfo)

### Index (cGgsnHistNotifIndex)

Monotonically increasing integer that indexes notifications. The value of this object is wrapped back to 1 when it reaches the maximum value of 4294967295.

### Type of Notification (cGgsnHistNotifType)

Type of notification issued by the device. Type can be:

Type | Description
ggsnServiceUp (1) | GGSN service started
ggsnServiceDown (2) | GGSN service shut down
mapSgsnUp (3) | MAP-SGSN service started
mapSgsnDown (4) | MAP-SGSN service shut down
noResource (5) | MS initiated or network initiated PDP count reached limit
noRadius (6) | Radius server not configured
noDHCPServer (7) | DHCP server not configured
ipAllocationFail (8) | IP address allocation failed
authenticationFail (9) | Authentication failed
apnUnreachable (10) | Access point not reachable

### Severity Level (cGgsnHistNotifSeverity)

Indicates the severity level of notification. You cannot set this object to cleared (1) or indeterminate (2).

### Notification Time (cGgsnHistNotifTimestamp)

Value of sysUpTime when the notification was generated.

### Address Reachable (cGgsnHistNotifGgsnIpAddrType)

Type of Internet address by which cGgsnHistNotifGgsnIpAddr can be reached.

### Device that generated Notification (cGgsnHistNotifGgsnIpAddr)

IP address that uniquely identifies the device that generated the notification.

### Additional Type Information (cGgsnHistNotifInfo)

Textual description of cGgsnHistNotifType. This object contains information about the alarm type. This object could also contain additional information.

If the message text exceeds 64 bytes, the message is truncated to 63 bytes and an asterisk (*) is appended to show that the message has been truncated.