# Ethernet Packet Anomalies

The CiscoView Monitor Port dialog box displays the following status information for an Ethernet port:

Small Pkts (locIfInRunts)

Large Pkts (locIfInGiants)

Misaligned Pkts (locIfInFrame)

Small Pkts (locIfInRunts)

Number of input packets that were smaller than the physical media permitted.

Misaligned Pkts (locIfInFrame)

Number of input packets that were misaligned.

Large Pkts (locIfInGiants)

Number of input packets that were larger than the physical media permitted.