# GGSN Aggregate Routes Table

From this dialog box, you can view the GGSN aggregate routes table.

Note: This dialog box is available only if the value of cGtpGSNService is set to ggsn.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select GGSN Aggregate Routes Table from the Category drop-down box.

The following information is displayed:

> Default Address Type (cGgsnDefaultAggregIpAddrType)

> Default IP Address (cGgsnDefaultAggregIpAddr)

> Default IP Address Mask (cGgsnDefaultAggregIpMask)

> Create/Delete Row (cGgsnDefaultAggregRowStatus)

### Default Address Type (cGgsnDefaultAggregIpAddrType)

Type of Internet address denoted by cGgsnDefaultAggregIpAddr.

### Default IP Address (cGgsnDefaultAggregIpAddr)

IP address whose network prefix is defined by cGgsnDefaultAggregIpMask.

### Default IP Address Mask (cGgsnDefaultAggregIpMask)

Net mask pertaining to cGgsnDefaultAggregIpAddr.

### Create/Delete Row (cGgsnDefaultAggregRowStatus)

Status of the table entry. Change the status to create a new table entry or delete an existing one.

- To create a row, set the object to createAndGo.

- To delete a row, set the object to destroy.

Note: The values createAndWait and notInService are not supported.