# GGSN History Table

From this dialog box, you can view the GGSN notification history table.

Note: This dialog box is available only if the value of cGtpGSNService is set to ggsn.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select GGSN History Table from the Category drop-down box.

The following information is displayed:

> Index (cGgsnHistNotifIndex)

> Type of Notification (cGgsnHistNotifType)

> Severity Level (cGgsnHistNotifSeverity)

> Notification Time (cGgsnHistNotifTimestamp)

> Address Reachable (cGgsnHistNotifGgsnIpAddrType)

> Device that generated Notification (cGgsnHistNotifGgsnIpAddr)

> Additional Type Information (cGgsnHistNotifInfo)

### Index (cGgsnHistNotifIndex)

Monotonically increasing integer that indexes notifications. The value of this object is wrapped back to 1 when it reaches the maximum value of 4294967295.

### Type of Notification (cGgsnHistNotifType)

Type of notification issued by the device. There are 10 possible values:

Type | Description
ggsnServiceUp (1) | GGSN service started
ggsnServiceDown (2) | GGSN service shut down
mapSgsnUp (3) | MAP-SGSN service started
mapSgsnDown (4) | MAP-SGSN service shut down
noResource (5) | MS initiated or network initiated PDP count reached limit
noRadius (6) | Radius server not configured
noDHCPServer (7) | DHCP server not configured
ipAllocationFail (8) | IP address allocation failed
authenticationFail (9) | Authentication failed
apnUnreachable (10) | Access point not reachable

### Severity Level (cGgsnHistNotifSeverity)

Indicates the severity level of the notification. There are seven possible values:

cleared(1) | minor(5)
indeterminate(2) | warning(6)
critical(3) | info(7)
major(4) |

Note: You cannot set this object to cleared(1) or indeterminate(2).

### Notification Time (cGgsnHistNotifTimestamp)

Value of sysUpTime when the notification was generated.

### Address Reachable (cGgsnHistNotifGgsnIpAddrType)

Type of Internet address by which cGgsnHistNotifGgsnIpAddr can be reached. There are six possible values:

> unknown(0)

> ipv4(1)

> ipv6(2)

> ipv4z(3)

> ipv6z(4)

> dns(16)

### Device that generated Notification (cGgsnHistNotifGgsnIpAddr)

IP address that uniquely identifies the device that generated the notification.

### Additional Type Information (cGgsnHistNotifInfo)

Textual description of cGgsnHistNotifType. This object contains information about the alarm type. This object could also contain additional information.

If the message text exceeds 64 bytes, the message is truncated to 63 bytes and an asterisk (*) is appended to show that the message has been truncated.