# Banner Configuration

WSC-6500-SFM card liquid crystal display (LCD) banner>Configure

This dialog box provides information on LCD Banner Configuration.

To view the definition for a particular MIB variable, click the appropriate link from the following list:

- Banner Index

- LCD Banner

- Banner Max Size

The following list specifies buttons in this dialog box, as well as their function:

- Click OK to continue.

- Click Apply to make changes take effect.

- Click Cancel to close the dialog box.

- Click Refresh to reload the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access the online help.

Banner Index (cc6kxbarLcdBannerIndex)

Object which specifies a unique entry in the table.

LCD Banner (cc6kxbarLcdBannerBanner)

Message that would be displayed on the fabric card LCD.

Note: The size of cc6kxbarLcdBannerBanner should not be greater than cc6kxbarLcdBannerMaxSize value.

Banner Max Size (cc6kxbarLcdBannerMaxSize)

Maximum size of the cc6kxbarLcdBannerBanner.