# CDMA PDSN PCF Table

This dialog box is applicable to Member and Peer to Peer clusters.

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Configure.

3. Select CDMA PDSN PCF Table.

### PCF Ip Address (cCdmaPcfIpAddress)

IP address identifying a packet control function (PCF).