# Configuring Routers for Flash File Administration

To configure a core router for flash file administration, set parameters with the following IOS configuration commands:

ip rcmd rcp-enable

ip rcmd rsh-enable

ip rcmd remote-host local-user remote-host remote-user enable

snmp-server system-shutdown

snmp-server community community-string RW

You must also configure the network management workstation.