# GGSN Access Point Violation and Redirection

From this dialog box, you can view access point violation and intermobile redirection statistics.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Statistics.

4. Select GGSN Access Point Statistics from the Category drop-down box.

5. With an entry selected in the GGSN Access Point Statistics dialog box, click Monitor.

6. Select the category GGSN Access Point Violation and Redirection.

The following information is displayed:

> Source Address Violation (cgprsAccPtSourceAddrViolTpdus)

> Destination Address Violation (cgprsAccPtDestAddrViolTpdus)

> Redirected InterMobile Communication (cgprsAccPtRedirInterMobilTraffic)

### Source Address Violation (cgprsAccPtSourceAddrViolTpdus)

Number of upstream TPDUs (Payload of GPRS Tunneling Protocol) that have been dropped due to source address violation as specified by cgprsAccPtVerifyUpStrTpduSrcAddr.

### Destination Address Violation (cgprsAccPtDestAddrViolTpdus)

Number of upstream TPDUs that have been dropped due to destination address violation as specified by cgprsAccPtVerifyUpStrTpduDstAddr.

### Redirected InterMobile Communication (cgprsAccPtRedirInterMobilTraffic)

Number of packets, pertaining to intermobile communication, that have been redirected to the device specified by cgprsAccPtRedirInterMobilAddr.