# Mobile Router Configs

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Configure button.

4. Select category Mobile Router Configs.

The following information appears:

> Collocated Tunnel Indication (cmiMrCollocatedTunnel)

### Collocated Tunnel Indication (cmiMrCollocatedTunnel)

Indicates whether a single tunnel or dual tunnels will be created between a mobile router and a home agent when the mobile router registers with a CCoA.